Release note:

LevelOne IGP-1271 (Hardware version:1)
LevelOne IGU-1271 (Hardware version:1)

Release version: v7.10.3199

-----------------------------------------

Firmware Version : v7.10.2799 ~ v7.10.3199

[CM Modification]
==============================================================
*S2025091601 - The cloud server is no longer under maintenance, disable Switch2go, TSOnline, APS for invalid functions.
*PM2023103101 - Adjust the "PoE Device Status" register judgment method to avoid VOP problems.
*S2023073101 - Remove IPMC warning messages from logfile.
*PM2023011201 - Modify PD Class display method when using Non-Standard PD (ex. Legacy mode)
*PM2021101901 - Adjust the limitation on Ethernet Type of ACL , to let all IPv4/v6 frames be treated as ether type frames.
 
[Fixed]
==============================================================
*Bug 24979 - GN and CM Typo in the SNMP/Trap Configuration trap detail page.
*Bug 25201 - The configurable range for the SNMP ICMPv6 Ping Egress Interface is inconsistent with the WEB.
*Bug 23987 - The IP configuration settings not success after configure on first wizard.
*Bug 24129 - Management IP address of connected node is not showing in LLDP neighbor info on neighbor node when there is no interface VLAN 1 IP address.
*Bug 24523 - PoE Status will show "PoE turned OFF - PD overload"
*Bug 23438 - The configured terminal exec-timeout of line vty will be reset after remote login.
*Bug 23500 - If receive ntp server information in both DHCPv4 and DHCPv6, there is only one server can be registered on ntp status table.
*Bug 23512 - If receive multiple ntp server through DHCPv4, there is only one server can be registered on ntp status table.
*Bug 23514 - If receive multiple dns servers through DHCPv4, the ip address of all of the dns servers is same.
*Bug 23521 - Tx Discard packets are not counting in the output of "show interface GigabitEthernet * statistics discard".
*Bug 23522 - When do write memory by reload warm, the write memory log isn't saved in logging flash.
*Bug 23523 - Interface of DDMI information isn't displaying correctly in logging flash(non-volatile syslog).
*Bug 23596 - Unable delete vlan 1 from web.
*Bug 23616 - Change auto-logout time will occur force logout.
*Bug 23629 - Can't be removed VLAN 1 via CLI.
*Bug 23402 - Device name cannot be changed in the DMS.
*Bug 22721 - Using privilege 15 of user to login the switch, sometimes the prompt shows ">" and privilege is wrong.
*Bug 22897 - The time of syslog is still getting changed if system time is changed.
*Bug 22896 - System time is around 1 seconds delay in every minute when inserting SFP module with DDM function.
*Bug 23048 - Switch will crash when performing save start via SNMP twice quickly.
*Bug 23030 - DHCP client cannot get ip when enable DHCP relay.
*Bug 23073 - LLDP Neighbor can not show ORING switch information.
*Bug 22719 - Switch will crash if repeatedly login/out via ssh quickly.
*Bug 23272 - Unregistered IPMCv4 Flooding control should only take effect when IGMP Snooping is enabled.
*Bug 21688 - DDM information are not updated.
*Bug 21750 - Rapid Chain function is not as expected.
*Bug 21778 - PMD auto-negotiation advertised capability information is wrong in the LLDP packet of fiber ports.
*Bug 22031 - SNMP Trap Security Engine ID all F or 0 can be entered in Web_UI.
*Bug 22116 - DUT can not forward DHCP DISCOVER.
*Bug 22111 - When power reset the fiber can not link.
*Bug 22475 - Sifos pwron_pwrcap test is failed.
*Bug 22565 - Some descriptions are missing in the CLI.
*Bug 22558 - Missing description on clear ptp and mep client in CLI.
*Bug 22576 - Some descriptions are missing in the CLI.
*Bug 22608 - Some descriptions are missing in the CLI.
*Bug 22588 - Event group Auth-Fail trap shows incorrect message.
*Bug 22594 - If PoE MCU upgrade same version ,the DUT should show message "PoE firmware had already been upgraded." and block upgrade process.
*Bug 22595 - Poe Request/Allocate Pwr with LLDP PoE Power information are inconsistent by LLDP protocol.
*Bug 22605 - Should remove PoE status "Capacitor Detection" field in CLI.
 
[NOTE]
==============================================================
*To verify modifications, please follow the steps below after upgrading FW.
- Connect to console port.
- Login device via CLI.
- Type Command "reload defaults".
- Type Command "copy running-config startup-config".
- Reboot device.